**HOT WORK PERMIT**

|  |  |  |  |
| --- | --- | --- | --- |
| **Date of Issue** |       | **Valid from / to** |       |
| 1. **WORKER DETAILS**
 |
| **Hot Work undertaken by** |       | **Phone Number** |       |
| 1. **PROJECT / WORKS DETAILS**
 |
| **Location of work** |       |
| **Planned work activity** |       |
| 1. **ISOLATIONS REQUIRED**
 |
| **[ ]**  | **Essential Services (gas, water, electricity)** | **[ ]**  | **Fire Indicator Panel** | **[ ]**  | **Fire Supression Systems** |
| 1. **GENERAL WORK CONTROLS**
 |
| **Controls (Identify those general Hot Work & Ignition controls to be undertaken as part of the Hot Work)** | **Yes** | **NA** |
| Fire extinguishers supplied by are to be located immediately adjacent to the Hot Work area and within fifteen (15) metre of the work to be carried out  | **[ ]**  | **[ ]**  |
| Position Catch mats or boards over grid-mesh, flooring, or grates to catch sparks, slag, or other hot debris. Spark and flash screens are in place. | **[ ]**  | **[ ]**  |
| Drains, cable racks, electrical cables and other heat/fire sensitive items are covered | **[ ]**  | **[ ]**  |
| If working outdoors, the area has been wetted down prior to work commencing and water is available and onsite if required.  | **[ ]**  | **[ ]**  |
| One (1) metre clearance to any insulated sandwich panel (otherwise relocate work or provide thermal barrier). | **[ ]**  | **[ ]**  |
| A four (4) metre cleared space around and above the area where Hot Work is to be performed. | **[ ]**  | **[ ]**  |
| The worksite has been isolated and traffic/pedestrian movement restricted. | **[ ]**  | **[ ]**  |
| Is the wind direction satisfactory for Hot Work to be done | **[ ]**  | **[ ]**  |
| Is Hot Work Activity located at a level which has the potential for a fall hazard (Working at Heights Permit to be used in conjunction with Hot Work Permit) | **[ ]**  | **[ ]**  |
| 1. **COMPLETION SIGN OFF**
 |
| **Fire Watch** | A continuous fire watch must be provided during and for a minimum of 30 minutes after work, after which periodic checks are required for a further 60 minutes (with checks undertaken every 10-15 minutes). |
| **Name** |       | **Signature** |       |
| **Completion date / time** |       |